signal aorb : std\_logic;

aorb <= i\_A or i\_B;

o\_SD <= aorb or i\_Cin;